Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSerial_SetSelcomDelay | ( | GoSerial | serial,
|  | k64u | delay
| ) |  |

Sets the delay from exposure until output is triggered, in units based on GoDomain.

mm units when GoDomain is distance, uS units when GoDomain is time.

Version
  Introduced in firmware 4.4.4.14

Parameters

  serial | GoSerial object.
  delay | k64s object.

Returns
  Operation status.