Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoControl_Open | ( | GoControl | control,
|  | kIpAddress | address,
|  | k32u | controlPort,
|  | k32u | upgradePort
| ) |  |

Opens connections to the specified sensor IP address.

The Open function immediately opens a control connection. Later, while in the open state, if an upgrade command is given, an upgrade connection will be established automatically at that time.

Version
  Introduced in firmware 4.8.2.76

Parameters

  control | GoControl object.
  address | Sensor IP address.
  controlPort | Control Port
  upgradePort | Upgrade Port

Returns
  Operation status.