Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages
GoAdvanced.h
1 /// @cond (Gocator_1x00 || Gocator_2x00)
2
3 /**
4 * @file GoAdvanced.h
5 * @brief Declares the GoAdvanced class.
6 *
7 * @internal
8 * Copyright (C) 2016-2018 by LMI Technologies Inc.
9 * Licensed under the MIT License.
10 * Redistributed files must retain the above copyright notice.
11 */
12 #ifndef GO_ADVANCED_H
13 #define GO_ADVANCED_H
14
15 #include <GoSdk/GoSdkDef.h>
16
17 kBeginHeader()
18
19 /**
20 * @class GoAdvanced
21 * @extends kObject
22 * @ingroup GoSdk
23 * @brief Represents configurable advanced acquisition settings.
24 */
25 typedef kObject GoAdvanced;
26
27 /**
28 * Sets the advanced acquisition type.
29 *
30 * @public @memberof GoAdvanced
31 * @version Introduced in firmware 4.6.1.140
32 * @param advanced GoAdvanced object.
33 * @param type The advanced type to set.
34 * @return Operation status.
35 */
36 GoFx(kStatus) GoAdvanced_SetType(GoAdvanced advanced, GoAdvancedType type);
37
38 /**
39 * Returns the user defined advanced acquisition type.
40 *
41 * @public @memberof GoAdvanced
42 * @version Introduced in firmware 4.6.1.140
43 * @param advanced GoAdvanced object.
44 * @return The advanced type.
45 */
46 GoFx(GoAdvancedType) GoAdvanced_Type(GoAdvanced advanced);
47
48 /**
49 * Returns a boolean relating to whether the user defined advanced acquisition type value will be used by the system.
50 *
51 * @public @memberof GoAdvanced
52 * @version Introduced in firmware 4.6.1.140
53 * @param advanced GoAdvanced object.
54 * @return kTRUE if the user defined advanced type will be used and kFALSE otherwise.
55 */
56 GoFx(kBool) GoAdvanced_IsTypeUsed(GoAdvanced advanced);
57
58 /**
59 * Returns the advanced acquisition type to be used by the system.
60 *
61 * @public @memberof GoAdvanced
62 * @version Introduced in firmware 4.6.1.140
63 * @param advanced GoAdvanced object.
64 * @return The system value advanced type.
65 */
66 GoFx(GoAdvancedType) GoAdvanced_TypeSystemValue(GoAdvanced advanced);
67
68 /**
69 * Sets the spot threshold.
70 *
71 * @public @memberof GoAdvanced
72 * @version Introduced in firmware 4.6.1.140
73 * @param advanced GoAdvanced object.
74 * @param value Spot threshold.
75 * @return Operation status.
76 */
77 GoFx(kStatus) GoAdvanced_SetSpotThreshold(GoAdvanced advanced, k32u value);
78
79 /**
80 * Returns the user defined spot threshold.
81 *
82 * @public @memberof GoAdvanced
83 * @version Introduced in firmware 4.6.1.140
84 * @param advanced GoAdvanced object.
85 * @return The spot threshold.
86 */
87 GoFx(k32u) GoAdvanced_SpotThreshold(GoAdvanced advanced);
88
89 /**
90 * Returns the minimum spot threshold limit.
91 *
92 * @public @memberof GoAdvanced
93 * @version Introduced in firmware 4.6.1.140
94 * @param advanced GoAdvanced object.
95 * @return The minimum spot threshold.
96 */
97 GoFx(k32u) GoAdvanced_SpotThresholdLimitMin(GoAdvanced advanced);
98
99 /**
100 * Returns the maximum spot threshold limit.
101 *
102 * @public @memberof GoAdvanced
103 * @version Introduced in firmware 4.6.1.140
104 * @param advanced GoAdvanced object.
105 * @return The maximum spot threshold.
106 */
107 GoFx(k32u) GoAdvanced_SpotThresholdLimitMax(GoAdvanced advanced);
108
109 /**
110 * Returns a boolean value representing whether the user specified spot threshold value is used.
111 *
112 * @public @memberof GoAdvanced
113 * @version Introduced in firmware 4.6.1.140
114 * @param advanced GoAdvanced object.
115 * @return kTRUE if it is used and kFALSE otherwise.
116 */
117 GoFx(kBool) GoAdvanced_IsSpotThresholdUsed(GoAdvanced advanced);
118
119 /**
120 * Returns the system spot threshold value.
121 *
122 * @public @memberof GoAdvanced
123 * @version Introduced in firmware 4.6.1.140
124 * @param advanced GoAdvanced object.
125 * @return The system spot threshold.
126 */
127 GoFx(k32u) GoAdvanced_SpotThresholdSystemValue(GoAdvanced advanced);
128
129 /**
130 * Sets the maximum spot width.
131 *
132 * @public @memberof GoAdvanced
133 * @version Introduced in firmware 4.6.1.140
134 * @param advanced GoAdvanced object.
135 * @param value Maximum spot width.
136 * @return Operation status.
137 */
138 GoFx(kStatus) GoAdvanced_SetSpotWidthMax(GoAdvanced advanced, k32u value);
139
140 /**
141 * Returns the user defined maximum spot width.
142 *
143 * @public @memberof GoAdvanced
144 * @version Introduced in firmware 4.6.1.140
145 * @param advanced GoAdvanced object.
146 * @return The maximum spot width.
147 */
148 GoFx(k32u) GoAdvanced_SpotWidthMax(GoAdvanced advanced);
149
150 /**
151 * Returns the maximum spot width minimum limit.
152 *
153 * @public @memberof GoAdvanced
154 * @version Introduced in firmware 4.6.1.140
155 * @param advanced GoAdvanced object.
156 * @return The maximum spot width minimum limit.
157 */
158 GoFx(k32u) GoAdvanced_SpotWidthMaxLimitMin(GoAdvanced advanced);
159
160 /**
161 * Returns the maximum spot width maximum limit.
162 *
163 * @public @memberof GoAdvanced
164 * @version Introduced in firmware 4.6.1.140
165 * @param advanced GoAdvanced object.
166 * @return The maximum spot width maximum limit.
167 */
168 GoFx(k32u) GoAdvanced_SpotWidthMaxLimitMax(GoAdvanced advanced);
169
170 /**
171 * Returns a boolean relating to whether the user defined spot width max value will be used by the system.
172 *
173 * @public @memberof GoAdvanced
174 * @version Introduced in firmware 4.6.1.140
175 * @param advanced GoAdvanced object.
176 * @return kTRUE if the user value will be used and kFALSE otherwise.
177 */
178 GoFx(kBool) GoAdvanced_IsSpotWidthMaxUsed(GoAdvanced advanced);
179
180 /**
181 * Returns the maximum spot width system value.
182 *
183 * @public @memberof GoAdvanced
184 * @version Introduced in firmware 4.6.1.140
185 * @param advanced GoAdvanced object.
186 * @return The maximum spot width system value.
187 */
188 GoFx(k32u) GoAdvanced_SpotWidthMaxSystemValue(GoAdvanced advanced);
189
190 /**
191 * Returns the number of spot selection type options.
192 *
193 * @public @memberof GoAdvanced
194 * @version Introduced in firmware 4.6.1.140
195 * @param advanced GoAdvanced object.
196 * @return The spot selection type option count.
197 */
198 GoFx(kSize) GoAdvanced_SpotSelectionTypeOptionCount(GoAdvanced advanced);
199
200 /**
201 * Returns the spot selection type option at the given index.
202 *
203 * @public @memberof GoAdvanced
204 * @version Introduced in firmware 4.6.1.140
205 * @param advanced GoAdvanced object.
206 * @param index The option list index to access.
207 * @return The spot selection type option at the given index.
208 */
209 GoFx(GoSpotSelectionType) GoAdvanced_SpotSelectionTypeOptionAt(GoAdvanced advanced, kSize index);
210
211 /**
212 * Sets the spot selection type.
213 *
214 * @public @memberof GoAdvanced
215 * @version Introduced in firmware 4.6.1.140
216 * @param advanced GoAdvanced object.
217 * @param type Spot selection type.
218 * @return Operation status.
219 */
220 GoFx(kStatus) GoAdvanced_SetSpotSelectionType(GoAdvanced advanced, GoSpotSelectionType type);
221
222 /**
223 * Returns the user defined spot selection type.
224 *
225 * @public @memberof GoAdvanced
226 * @version Introduced in firmware 4.6.1.140
227 * @param advanced GoAdvanced object.
228 * @return The maximum spot width.
229 */
230 GoFx(GoSpotSelectionType) GoAdvanced_SpotSelectionType(GoAdvanced advanced);
231
232 /**
233 * Returns a boolean relating to whether the user defined spot selection type will be used by the system.
234 *
235 * @public @memberof GoAdvanced
236 * @version Introduced in firmware 4.6.1.140
237 * @param advanced GoAdvanced object.
238 * @return kTRUE if the user value will be used and kFALSE otherwise.
239 */
240 GoFx(kBool) GoAdvanced_IsSpotSelectionTypeUsed(GoAdvanced advanced);
241
242 /**
243 * Returns the system spot selection type.
244 *
245 * @public @memberof GoAdvanced
246 * @version Introduced in firmware 4.6.1.140
247 * @param advanced GoAdvanced object.
248 * @return System spot selection type.
249 */
250 GoFx(GoSpotSelectionType) GoAdvanced_SpotSelectionTypeSystemValue(GoAdvanced advanced);
251
252 /**
253 * Returns the minimum segment size used in continuity sorting spot detection.
254 *
255 * @public @memberof GoAdvanced
256 * @version Introduced in firmware 4.6.2.79
257 * @param advanced GoAdvanced object.
258 * @return Minimum segment size
259 */
260 GoFx(k32u) GoAdvanced_SpotContinuityMinimumSegmentSize(GoAdvanced advanced);
261
262 /**
263 * Sets the minimum segment size used in continuity sorting spot detection.
264 *
265 * @public @memberof GoAdvanced
266 * @version Introduced in firmware 4.6.2.79
267 * @param advanced GoAdvanced object.
268 * @param value Minimum Segment Size.
269 * @return Operation status.
270 */
271 GoFx(kStatus) GoAdvanced_SetSpotContinuityMinimumSegmentSize(GoAdvanced advanced, k32u value);
272
273 /**
274 * Returns the search window size in the X direction used in continuity sorting spot detection.
275 *
276 * @public @memberof GoAdvanced
277 * @version Introduced in firmware 4.6.2.79
278 * @param advanced GoAdvanced object.
279 * @return Search window X dimension
280 */
281 GoFx(k32u) GoAdvanced_SpotContinuitySearchWindowX(GoAdvanced advanced);
282
283 /**
284 * Sets the search window size in the X direction used in continuity sorting spot detection.
285 *
286 * @public @memberof GoAdvanced
287 * @version Introduced in firmware 4.6.2.79
288 * @param advanced GoAdvanced object.
289 * @param value Search window X dimension.
290 * @return Operation status.
291 */
292 GoFx(kStatus) GoAdvanced_SetSpotContinuitySearchWindowX(GoAdvanced advanced, k32u value);
293
294 /**
295 * Returns the search window size in the Y direction used in continuity sorting spot detection
296 *
297 * @public @memberof GoAdvanced
298 * @version Introduced in firmware 4.6.2.79
299 * @param advanced GoAdvanced object.
300 * @return Search window Y dimension
301 */
302 GoFx(k32u) GoAdvanced_SpotContinuitySearchWindowY(GoAdvanced advanced);
303
304 /**
305 * Sets the search window size in the Y direction used in continuity sorting spot detection
306 *
307 * @public @memberof GoAdvanced
308 * @version Introduced in firmware 4.6.2.79
309 * @param advanced GoAdvanced object.
310 * @param value Search window Y dimension.
311 * @return Operation status.
312 */
313 GoFx(kStatus) GoAdvanced_SetSpotContinuitySearchWindowY(GoAdvanced advanced, k32u value);
314
315 /**
316 * Sets the analog camera gain.
317 *
318 * @public @memberof GoAdvanced
319 * @version Introduced in firmware 4.6.1.140
320 * @param advanced GoAdvanced object.
321 * @param value Analog camera gain.
322 * @return Operation status.
323 */
324 GoFx(kStatus) GoAdvanced_SetCameraGainAnalog(GoAdvanced advanced, k64f value);
325
326 /**
327 * Returns the user defined analog camera gain value.
328 *
329 * @public @memberof GoAdvanced
330 * @version Introduced in firmware 4.6.1.140
331 * @param advanced GoAdvanced object.
332 * @return Analog camera gain value.
333 */
334 GoFx(k64f) GoAdvanced_CameraGainAnalog(GoAdvanced advanced);
335
336 /**
337 * Returns the analog camera gain minimum value limit.
338 *
339 * @public @memberof GoAdvanced
340 * @version Introduced in firmware 4.6.1.140
341 * @param advanced GoAdvanced object.
342 * @return Analog camera gain minimum value limit.
343 */
344 GoFx(k64f) GoAdvanced_CameraGainAnalogLimitMin(GoAdvanced advanced);
345
346 /**
347 * Returns the analog camera gain maximum value limit.
348 *
349 * @public @memberof GoAdvanced
350 * @version Introduced in firmware 4.6.1.140
351 * @param advanced GoAdvanced object.
352 * @return Analog camera gain maximum value limit.
353 */
354 GoFx(k64f) GoAdvanced_CameraGainAnalogLimitMax(GoAdvanced advanced);
355
356 /**
357 * Returns a boolean value representing whether the user defined analog camera gain is used.
358 *
359 * @public @memberof GoAdvanced
360 * @version Introduced in firmware 4.6.1.140
361 * @param advanced GoAdvanced object.
362 * @return kTRUE if the user defined analog camera gain is used and kFALSE otherwise.
363 */
364 GoFx(kBool) GoAdvanced_IsCameraGainAnalogUsed(GoAdvanced advanced);
365
366 /**
367 * Returns the analog camera gain system value.
368 *
369 * @public @memberof GoAdvanced
370 * @version Introduced in firmware 4.6.1.140
371 * @param advanced GoAdvanced object.
372 * @return The analog camera gain system value.
373 */
374 GoFx(k64f) GoAdvanced_CameraGainAnalogSystemValue(GoAdvanced advanced);
375
376 /**
377 * Sets the digital camera gain
378 *
379 * @public @memberof GoAdvanced
380 * @version Introduced in firmware 4.6.1.140
381 * @param advanced GoAdvanced object.
382 * @param value Digital camera gain.
383 * @return Operation status.
384 */
385 GoFx(kStatus) GoAdvanced_SetCameraGainDigital(GoAdvanced advanced, k64f value);
386
387 /**
388 * Returns the user defined digital camera gain value.
389 *
390 * @public @memberof GoAdvanced
391 * @version Introduced in firmware 4.6.1.140
392 * @param advanced GoAdvanced object.
393 * @return The digital camera gain system value.
394 */
395 GoFx(k64f) GoAdvanced_CameraGainDigital(GoAdvanced advanced);
396
397 /**
398 * Returns the digital camera gain minimum value limit.
399 *
400 * @public @memberof GoAdvanced
401 * @version Introduced in firmware 4.6.1.140
402 * @param advanced GoAdvanced object.
403 * @return Digital camera gain minimum value limit.
404 */
405 GoFx(k64f) GoAdvanced_CameraGainDigitalLimitMin(GoAdvanced advanced);
406
407 /**
408 * Returns the digital camera gain maximum value limit.
409 *
410 * @public @memberof GoAdvanced
411 * @version Introduced in firmware 4.6.1.140
412 * @param advanced GoAdvanced object.
413 * @return Digital camera gain maximum value limit.
414 */
415 GoFx(k64f) GoAdvanced_CameraGainDigitalLimitMax(GoAdvanced advanced);
416
417 /**
418 * Returns a boolean value representing whether the user's digital camera gain value is used by the system.
419 *
420 * @public @memberof GoAdvanced
421 * @version Introduced in firmware 4.6.1.140
422 * @param advanced GoAdvanced object.
423 * @return kTRUE if used and kFALSE otherwise.
424 */
425 GoFx(kBool) GoAdvanced_IsCameraGainDigitalUsed(GoAdvanced advanced);
426
427 /**
428 * Returns the system's digital camera gain value.
429 *
430 * @public @memberof GoAdvanced
431 * @version Introduced in firmware 4.6.1.140
432 * @param advanced GoAdvanced object.
433 * @return Digital camera gain system value.
434 */
435 GoFx(k64f) GoAdvanced_CameraGainDigitalSystemValue(GoAdvanced advanced);
436
437 /**
438 * Sets the dynamic sensitivity.
439 *
440 * @public @memberof GoAdvanced
441 * @version Introduced in firmware 4.6.1.140
442 * @param advanced GoAdvanced object.
443 * @param value Dynamic sensitivity.
444 * @return Operation status.
445 */
446 GoFx(kStatus) GoAdvanced_SetDynamicSensitivity(GoAdvanced advanced, k64f value);
447
448 /**
449 * Returns the user defined dynamic sensitivity value.
450 *
451 * @public @memberof GoAdvanced
452 * @version Introduced in firmware 4.6.1.140
453 * @param advanced GoAdvanced object.
454 * @return User defined dynamic sensitivity value.
455 */
456 GoFx(k64f) GoAdvanced_DynamicSensitivity(GoAdvanced advanced);
457
458 /**
459 * Returns the dynamic sensitivity minimum value limit.
460 *
461 * @public @memberof GoAdvanced
462 * @version Introduced in firmware 4.6.1.140
463 * @param advanced GoAdvanced object.
464 * @return Dynamic sensitivity minimum value limit.
465 */
466 GoFx(k64f) GoAdvanced_DynamicSensitivityLimitMin(GoAdvanced advanced);
467
468 /**
469 * Returns the dynamic sensitivity maximum value limit.
470 *
471 * @public @memberof GoAdvanced
472 * @version Introduced in firmware 4.6.1.140
473 * @param advanced GoAdvanced object.
474 * @return Dynamic sensitivity maximum value limit.
475 */
476 GoFx(k64f) GoAdvanced_DynamicSensitivityLimitMax(GoAdvanced advanced);
477
478 /**
479 * Returns a boolean representing whether the user defined dynamic sensitivity value is used.
480 *
481 * @public @memberof GoAdvanced
482 * @version Introduced in firmware 4.6.1.140
483 * @param advanced GoAdvanced object.
484 * @return kTRUE if used and kFALSE otherwise.
485 */
486 GoFx(kBool) GoAdvanced_IsDynamicSensitivityUsed(GoAdvanced advanced);
487
488 /**
489 * Returns the dynamic sensitivity system value.
490 *
491 * @public @memberof GoAdvanced
492 * @version Introduced in firmware 4.6.1.140
493 * @param advanced GoAdvanced object.
494 * @return Dynamic sensitivity system value.
495 */
496 GoFx(k64f) GoAdvanced_DynamicSensitivitySystemValue(GoAdvanced advanced);
497
498 /**
499 * Sets the dynamic threshold.
500 *
501 * @public @memberof GoAdvanced
502 * @version Introduced in firmware 4.6.1.140
503 * @param advanced GoAdvanced object.
504 * @param value Dynamic threshold.
505 * @return Operation status.
506 */
507 GoFx(kStatus) GoAdvanced_SetDynamicThreshold(GoAdvanced advanced, k32u value);
508
509 /**
510 * Returns the dynamic threshold minimum value limit.
511 *
512 * @public @memberof GoAdvanced
513 * @version Introduced in firmware 4.6.1.140
514 * @param advanced GoAdvanced object.
515 * @return Dynamic threshold minimum value limit.
516 */
517 GoFx(k32u) GoAdvanced_DynamicThresholdLimitMin(GoAdvanced advanced);
518
519 /**
520 * Returns the dynamic threshold maximum value limit.
521 *
522 * @public @memberof GoAdvanced
523 * @version Introduced in firmware 4.6.1.140
524 * @param advanced GoAdvanced object.
525 * @return Dynamic threshold maximum value limit.
526 */
527 GoFx(k32u) GoAdvanced_DynamicThresholdLimitMax(GoAdvanced advanced);
528
529 /**
530 * Returns the user defined dynamic threshold value.
531 *
532 * @public @memberof GoAdvanced
533 * @version Introduced in firmware 4.6.1.140
534 * @param advanced GoAdvanced object.
535 * @return The user defined dynamic threshold value.
536 */
537 GoFx(k32u) GoAdvanced_DynamicThreshold(GoAdvanced advanced);
538
539 /**
540 * Returns a boolean representing whether or not the user defined dynamic threshold is used by the system.
541 *
542 * @public @memberof GoAdvanced
543 * @version Introduced in firmware 4.6.1.140
544 * @param advanced GoAdvanced object.
545 * @return Dynamic threshold minimum value limit.
546 */
547 GoFx(kBool) GoAdvanced_IsDynamicThresholdUsed(GoAdvanced advanced);
548
549 /**
550 * Returns the dynamic threshold system value.
551 *
552 * @public @memberof GoAdvanced
553 * @version Introduced in firmware 4.6.1.140
554 * @param advanced GoAdvanced object.
555 * @return Dynamic threshold system value.
556 */
557 GoFx(k32u) GoAdvanced_DynamicThresholdSystemValue(GoAdvanced advanced);
558
559 /**
560 * Sets the gamma type.
561 *
562 * @public @memberof GoAdvanced
563 * @version Introduced in firmware 4.6.1.140
564 * @param advanced GoAdvanced object.
565 * @param value Gamma type.
566 * @return Operation status.
567 */
568 GoFx(kStatus) GoAdvanced_SetGammaType(GoAdvanced advanced, GoGammaType value);
569
570 /**
571 * Returns the user defined gamma type.
572 *
573 * @public @memberof GoAdvanced
574 * @version Introduced in firmware 4.6.1.140
575 * @param advanced GoAdvanced object.
576 * @return User defined gamma type.
577 */
578 GoFx(GoGammaType) GoAdvanced_GammaType(GoAdvanced advanced);
579
580 /**
581 * Returns a boolean representing whether the user defined gamma type is used by the system.
582 *
583 * @public @memberof GoAdvanced
584 * @version Introduced in firmware 4.6.1.140
585 * @param advanced GoAdvanced object.
586 * @return kTRUE if used and kFALSE otherwise.
587 */
588 GoFx(kBool) GoAdvanced_IsGammaTypeUsed(GoAdvanced advanced);
589
590 /**
591 * Returns the system's gamma type value.
592 *
593 * @public @memberof GoAdvanced
594 * @version Introduced in firmware 4.6.1.140
595 * @param advanced GoAdvanced object.
596 * @return The system gamma type value.
597 */
598 GoFx(GoGammaType) GoAdvanced_GammaTypeSystemValue(GoAdvanced advanced);
599
600 /**
601 * Enables or disables senstivity compensation. NOTE: This is only applicable to
602 * 2300 B series sensors.
603 *
604 * @public @memberof GoAdvanced
605 * @version Introduced in firmware 4.6.1.140
606 * @param advanced GoAdvanced object.
607 * @param value kTRUE to enable and kFALSE to disable.
608 * @return Operation status.
609 */
610 GoFx(kStatus) GoAdvanced_EnableSensitivityCompensation(GoAdvanced advanced, kBool value);
611
612 /**
613 * Returns the user defined sensitivity compensation value.
614 *
615 * @public @memberof GoAdvanced
616 * @version Introduced in firmware 4.6.1.140
617 * @param advanced GoAdvanced object.
618 * @return User defined sensitivity compensation.
619 */
620 GoFx(kBool) GoAdvanced_SensitivityCompensationEnabled(GoAdvanced advanced);
621
622 /**
623 * Returns a boolean representing whether the user defined sensitivity compensation is used by the system.
624 *
625 * @public @memberof GoAdvanced
626 * @version Introduced in firmware 4.6.1.140
627 * @param advanced GoAdvanced object.
628 * @return kTRUE if used and kFALSE otherwise.
629 */
630 GoFx(kBool) GoAdvanced_IsSensitivityCompensationEnabledUsed(GoAdvanced advanced);
631
632 /**
633 * Returns the system's sensitivity compensation value.
634 *
635 * @public @memberof GoAdvanced
636 * @version Introduced in firmware 4.6.1.140
637 * @param advanced GoAdvanced object.
638 * @return kTRUE if enabled and kFALSE otherwise.
639 */
640 GoFx(kBool) GoAdvanced_SensitivityCompensationEnabledSystemValue(GoAdvanced advanced);
641
642 /**
643 * Sets surface engine encoding type (Default Standard)
644 *
645 * @public @memberof GoAdvanced
646 * @version Introduced in firmware 4.7.3.22
647 * @param advanced GoAdvanced object.
648 * @param encoding Surface Engine Encoding type
649 * @return Operation status.
650 */
651 GoFx(kStatus) GoAdvanced_SetSurfaceEncoding(GoAdvanced advanced, GoSurfaceEncoding encoding);
652
653 /**
654 * Returns the surface engine encoding type.
655 *
656 * @public @memberof GoAdvanced
657 * @version Introduced in firmware 4.7.3.22
658 * @param advanced GoAdvanced object.
659 * @return The Surface Engine Encoding type.
660 */
661 GoFx(GoSurfaceEncoding) GoAdvanced_SurfaceEncoding(GoAdvanced advanced);
662
663 /**
664 * Sets the phase filter type. (Default None)
665 *
666 * @public @memberof GoAdvanced
667 * @version Introduced in firmware 4.7.3.22
668 * @param advanced GoAdvanced object.
669 * @param phaseFilter Phase Filter type.
670 * @return Operation status.
671 */
672 GoFx(kStatus) GoAdvanced_SetSurfacePhaseFilter(GoAdvanced advanced, GoSurfacePhaseFilter phaseFilter);
673
674 /**
675 * Returns the phase filter type.
676 *
677 * @public @memberof GoAdvanced
678 * @version Introduced in firmware 4.7.3.22
679 * @param advanced GoAdvanced object.
680 * @return The phase filter type.
681 */
682 GoFx(GoSurfacePhaseFilter) GoAdvanced_SurfacePhaseFilter(GoAdvanced advanced);
683
684 kEndHeader()
685 #include <GoSdk/GoAdvanced.x.h>
686
687 #endif
688
689 /// @endcond
k32u
GoSurfacePhaseFilter
Represents a surface phase filter type.
kSize
GoSurfaceEncoding
Represents a surface scanning engine encoding type.
GoSdkDef.h
Essential SDK declarations.
GoGammaType
Represents an advanced gamma type.
kObject
kStatus
k64f
kBool