Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

GoDiscoveryOpMode GoDiscoveryExtInfo_OpMode | ( | GoDiscoveryExtInfo | msg | ) |

Gets the operational mode returned by the source device's main controller/host.

Indicates if the host is: a. a virtual sensor b. a standalone sensor c. a host accelerating a sensor

Version
  Introduced in firmware 5.1.6.0

Parameters

  msg | Message object.

Returns
  Operational mode.