Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

k64f GoLayout_MultiplexSingleExposureDuration | ( | GoLayout | layout | ) |

Returns a value representing the multiplexing exposure duration in a single device sensor configuration.

(microseconds)

Version
  Introduced in firmware 4.0.10.27

Parameters

  layout | GoLayout object.

Returns
  Single device multiplexing exposure duration.