Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSetup_SetTriggerExternalInputIndex | ( | GoSetup | setup,
|  | k32s | index
| ) |  |

Sets the external input index to trigger profile/surface capturing.

Version
  Introduced in firmware 5.1.3.14

Parameters

  setup | GoSetup object.
  index | External digital input index.

Returns
  Operation status.