Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages
GoSensorAccelStatus Struct Reference
GoSdk

## Description

Represents the acceleration status of a sensor that is being accelerated by the local host. The acceleration state state can be GO_SENSOR_ACCEL_STATE_AVAILABLE (while acceleration has not yet) or GO_SENSOR_ACCEL_STATE_ACCELERATED (acceleration completed). It is not applicable for a sensor being accelerated by another host (GO_SENSOR_ACCEL_STATE_ACCELERATED_BY_OTHER). These are applicable only when using the GoAcceleratorMgr class.

The following enumerators are defined:

- GO_SENSOR_ACCEL_STATUS_SUCCESS
- GO_SENSOR_ACCEL_STATUS_ACCELERATING
- GO_SENSOR_ACCEL_STATUS_DECELERATING
- GO_SENSOR_ACCEL_STATUS_FAIL_TO_ACCEL
- GO_SENSOR_ACCEL_STATUS_MISSING
- GO_SENSOR_ACCEL_STATUS_STOPPED

Inheritance diagram for GoSensorAccelStatus:

The documentation for this struct was generated from the following file:

- GoSdkDef.h