Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoControl_SetVoltage | ( | GoControl | control,
|  | GoVoltageSetting | voltage,
|  | k32u | cableLength
| ) |  |

Set sensor voltage settings (only on G3210)

Version
  Introduced in firmware 4.7.5.25

Parameters

  control | GoControl object.
  voltage | Either 48V or 24V operation
  cableLength | When in 24V operation mode the cable length (millimeters) must also be supplied

Returns
  Operation status.