Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSetup_SetExternalInputZPulseIndex | ( | GoSetup | setup,
|  | k32u | index
| ) |  |

Sets the external input index for triggering encoder Z-pulse.

Version
  Introduced in firmware 5.1.6.0

Parameters

  setup | GoSetup object.
  index | Index of external input to use.

Returns
  Operation status.