Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoGeoCal_ApplyActiveArea | ( | GoGeoCal | cal,
|  | k32u | x,
|  | k32u | y,
|  | k32u | width,
|  | k32u | height,
|  | k32u | xSubsampling,
|  | k32u | ySubsampling,
|  | kSize | cameraIndex
| ) |  |

Applies a new camera window to the camera orientation information and updates coefficients.

Version
  Introduced in firmware 5.1.6.0

Parameters

  cal | GoGeoCal object.
  x | X of new camera window.
  y | Y of new camera window.
  width | Width of new camera window.
  height | Height of new camera window.
  xSubsampling | X subsampling of new camera window.
  ySubsampling | Y subsampling of new camera window.
  cameraIndex | Camera index.

Returns
  Operation status.