Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSensor_StartRecordingStream | ( | GoSensor | sensor,
|  | kChar * | destFile
| ) |  |

Starts recording to a stream.

NOTE: Before calling this function, the sensor should already be running and recording. GoSensor_StopRecordingStream() should be called before executing any other sensor commands, with the exception of GoSensor_IsRecordingStreaming().

Version
  Introduced in firmware 4.6.4.66

Parameters

  sensor | GoSensor object.
  destFile | A local file path to store the .rec data.

Returns
  Operation status.