Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSetup_SetEncoderSpacing | ( | GoSetup | setup,
|  | k64f | period
| ) |  |

Sets the current encoder period for encoder-based triggering.

Version
  Introduced in firmware 4.0.10.27

Parameters

  setup | GoSetup object.
  period | Encoder period (mm).

Returns
  Operation status.