Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoCylinderRegion_SetX | ( | GoCylinderRegion | region,
|  | k64f | x
| ) |  |

Sets the X position.

Note
  Supported with G2, G3

Version
  Introduced in firmware 4.0.10.27

Parameters

  region | GoCylinderRegion object.
  x | The X position to set.(mm)

Returns
  Operation status.