Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoEthernet_SetAsciiControlPort | ( | GoEthernet | ethernet,
|  | k32u | port
| ) |  |

Sets the port number of the ASCII control port.

Version
  Introduced in firmware 4.0.10.27

Parameters

  ethernet | GoEthernet object.
  port | The selected ASCII control port value.

Returns
  Operation status.