Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

k32s GoSurfaceGenerationFixedLength_TriggerExternalInputIndex | ( | GoSurfaceGeneration | surface | ) |

Gets the external input index to trigger surface capturing.

Note
  Supported with G2, G3

Version
  Introduced in firmware 5.2.1.110

Parameters

  surface | GoSurfaceGeneration object.

Returns
  External input index to trigger capturing.