Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSensor_SetVoltage | ( | GoSensor | sensor,
|  | GoVoltageSetting | voltage,
|  | k64f | cableLength
| ) |  |

Set sensor voltage settings (only on G3210)

Version
  Introduced in firmware 4.7.5.25

Parameters

  sensor | GoSensor object.
  voltage | Either 48V or 24V operation
  cableLength | When in 24V operation mode the cable length (meter) must also be supplied

Returns
  Operation status.