Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

k64f GoSystem_MaxMinimumMultiplexPeriod | ( | GoSystem | system | ) |

Returns the maximum value of all multiplexed sensor's minimum multiplexing periods.

Note
  Supported with G1, G2

Version
  Introduced in firmware 4.0.10.27

Parameters

  system | GoSystem object.

Returns
  Operation status.