Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSensor_AccelSensorIpAddress | ( | GoSensor | sensor,
|  | kIpAddress * | ipAddress
| ) |  |

Returns the physical sensor IP address when sensor is accelerated.

Version
  Introduced in firmware 5.2.18.3

Parameters

  sensor | GoSensor object.
  ipAddress | Destination to store the IP Address.

Returns
  Operational status.