Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSensor_RestoreDefaults | ( | GoSensor | sensor,
|  | kBool | restoreAddress
| ) |  |

Restores factory default settings.

WARNING! This operation writes to flash storage. Review the user manual for implications.

Version
  Introduced in firmware 4.0.10.27

Parameters

  sensor | GoSensor object.
  restoreAddress | kTRUE to restore the factory default IP address; False otherwise.

Returns
  Operation status.

Remarks
  Calling this function will result in writing operations to flash storage. Should the process be disrupted due to power loss or other factors, the sensor may enter Rescue mode.