Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSystem_StartExposureAutoSet | ( | GoSystem | system | ) |

Performs exposure auto set for sensors in the ready state.

NOTE: This operation will result in sensor starts for the duration of the exposure AutoSet. A successful operation status does NOT modify the configuration. You must retrieve the resulting exposure values and set it for the appropriate exposure setting. This involves enabling the data connection prior to running exposure auto set and then receiving an exposure auto set message, which you can then use to query the status and access the resulting value.

Version
  Introduced in firmware 4.0.10.27

Parameters

  system | GoSystem object.

Returns
  Operation status.

See also
  GoSystem_EnableData, GoSystem_ReceiveData