Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSetup_SetAlignmentStationaryTarget | ( | GoSetup | setup,
|  | GoAlignmentTarget | target
| ) |  |

Sets the target type used for stationary alignment calibration.

Version
  Introduced in firmware 4.0.10.27

Parameters

  setup | GoSetup object.
  target | Alignment target type.

Returns
  Operation status.