Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoPartDetection_SetGapWidth | ( | GoPartDetection | detection,
|  | k64f | gap
| ) |  |

Sets the part detection gap width.

Note
  Supported with G2, G3

Version
  Introduced in firmware 4.0.10.27

Parameters

  detection | GoPartDetection object.
  gap | The part detection gap width value to set.(mm)

Returns
  Operation status.