Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoDiscovery_SetAddress | ( | GoDiscovery | discovery,
|  | k32u | deviceId,
|  | const GoAddressInfo * | address
| ) |  |

Configures a sensor's network address settings.

This function uses UDP broadcasts; the sensor and can be on a different subnet than the client.

The sensor will automatically reboot if the address is successfully changed.

Version
  Introduced in firmware 4.0.10.27

Parameters

  discovery | Discovery object.
  deviceId | Sensor device identifier (serial number).
  address | New address information.

Returns
  Operation status.