Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoAcceleratorMgr_SetPortRange | ( | GoAcceleratorMgr | manager,
|  | k16u | startPort,
|  | k16u | endPort
| ) |  |

Set the range of port numbers used to communicate with the accelerated sensors.

Changes to the port range is allowed only if no sensor is configured for acceleration. Changing the port range is optional if the client application can use the default port range. The port numbers range must be within the port range limits (see GoAcceleratorMgr_GetPortRangeLimits()). Configure the port range if your network places limits on what ports are permitted for communication use or if some range of ports is known to be used by another application.

Version
  Introduced in firmware 5.2.18.3

Parameters

  manager | GoAcceleratorMgr object.
  startPort | Starting port number in the range
  endPort | Last port number in the range.

Returns
  Operation status.