Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSetup_SetLaserIdleTime | ( | GoSetup | setup,
|  | k64u | time
| ) |  |

This API is experimental and may change in a future release Sets the time before the laser deactivates.

Version
  Introduced in firmware 4.8.2.76

Parameters

  setup | GoSetup object.
  time | idle time. (microseconds)

Returns
  Operation status.