Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoLayout_EnableMultiplexSingle | ( | GoLayout | layout,
|  | kBool | enabled
| ) |  |

Enables single sensor(not buddied) configuration multiplexing.

Note
  Supported with G1, G2

Version
  Introduced in firmware 4.0.10.27

Parameters

  layout | GoLayout object.
  enabled | kTRUE to enable, or kFALSE to disable.

Returns
  Operation status.