Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSensor_Timestamp | ( | GoSensor | sensor,
|  | k64u * | time
| ) |  |

Gets the current time stamp (common among all synchronized sensors).

Version
  Introduced in firmware 4.0.10.27

Parameters

  sensor | GoSensor object.
  time | Receives the current time stamp(us).

Returns
  Operation status.