Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoAnalog_SetDataScaleMin | ( | GoAnalog | analog,
|  | k64f | min
| ) |  |

Sets the measurement value associated with the minimum output current value.

Version
  Introduced in firmware 4.0.10.27

Parameters

  analog | GoAnalog object.
  min | Minimum measurement value (units are measurement dependent).

Returns
  Operation status.