Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoControl_BeginScheduledStart | ( | GoControl | control,
|  | k64s | value
| ) |  |

Sends a scheduled start command to a sensor with the currently selected input source, but doesn't wait for the response.

Use the GoControl_EndScheduledStart function to wait for the sensor's reply.

Version
  Introduced in firmware 4.1.3.106

Parameters

  control | GoControl object.
  value | Scheduled start value (in uS for time trigger and ticks for encoder trigger)

Returns
  Operation status.

See also
  GoControl_EndScheduledStart, GoControl_SetInputSource, GoControl_GetInputSource