Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages
Public Attributes
GoStates Struct Reference
GoSdk

## Description

Sensor state, login, alignment information, recording state, playback source, uptime, playback information, and auto-start setting state.

Inheritance diagram for GoStates:

## Public Attributes
GoAlignmentRef | alignmentReference
| The alignment reference of the sensor.
GoAlignmentState | alignmentState
| The alignment state of the sensor.
kBool | autoStartEnabled
| The auto-start enabled state.
GoBrandingType | brandingType
| The branding type of the sensor; (for brand customization schemes).
k32u | cableLength
| The length of the cable (in millimeters) from the Sensor to the Master.
kBool | isAccelerator
| The accelerated state of the sensor.
GoUser | loginType
| The logged in user.
k32u | playbackCount
| The playback count.
k32u | playbackPos
| The playback position index.
k32s | playbackSource
| The current playback source of the sensor.
kBool | quickEditEnabled
| The current state of editing.
kBool | recordingEnabled
| The current state of recording on the sensor.
GoSecurityLevel | security
| The security level setup on the sensor: none/basic; when basic level does not allow anonymous users accessing system.
GoState | sensorState
| The state of the sensor.
k32u | uptimeMicrosec
| Sensor uptime in microseconds.
k32u | uptimeSec
| Sensor uptime in seconds.
GoVoltageSetting | voltage
| Power Source Voltage: 24 or 48 V.

The documentation for this struct was generated from the following file:

- GoSdkDef.h