Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages
GoSensorAccelStatus Struct Reference
GoSdk

## Description

Represents the acceleration status of a sensor that is available or being accelerated by the local host. The corresponding acceleration state can be GO_SENSOR_ACCEL_STATE_AVAILABLE (while acceleration has not yet) or GO_SENSOR_ACCEL_STATE_ACCELERATED (acceleration completed). These status values are not applicable for a sensor accelerated by another host (ie. state is GO_SENSOR_ACCEL_STATE_ACCELERATED_BY_OTHER)). These statuses are applicable only when using the GoAcceleratorMgr class.

The following enumerators are defined:

- GO_SENSOR_ACCEL_STATUS_SUCCESS
- GO_SENSOR_ACCEL_STATUS_ACCELERATING
- GO_SENSOR_ACCEL_STATUS_DECELERATING
- GO_SENSOR_ACCEL_STATUS_MISSING
- GO_SENSOR_ACCEL_STATUS_STOPPED
- GO_SENSOR_ACCEL_STATUS_FAIL_TO_ACCEL
- GO_SENSOR_ACCEL_STATUS_STOPPED_AVAILABLE
- GO_SENSOR_ACCEL_STATUS_STOPPED_ACCELERATED_BY_OTHER
- GO_SENSOR_ACCEL_STATUS_STOPPED_FW_MISMATCH
- GO_SENSOR_ACCEL_STATUS_STOPPED_PORT_IN_USE
- GO_SENSOR_ACCEL_STATUS_STOPPED_UNREACHABLE

Inheritance diagram for GoSensorAccelStatus:

The documentation for this struct was generated from the following file:

- GoSdkDef.h