Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSystem_ScheduledStart | ( | GoSystem | system,
|  | k64s | value
| ) |  |

Starts all sensors that are currently in the ready state at a scheduled value.

NOTE: The value specified is the target value to start at, not a relative offset from the current value. The typical usage is to obtain the current value first, add an offset to it, and start at that value.

Version
  Introduced in firmware 4.1.3.106

Parameters

  system | GoSystem object.
  value | The value at which to start the sensor. It is in uS when time triggered and ticks when encoder triggered.

Returns
  Operation status.

See also
  GoSystem_Stop, GoSensor_ScheduledStart, GoSensor_Stop, GoSetup_SetTriggerSource, GoSetup_TriggerSource