Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoLayout_EnableMultiplexBuddy | ( | GoLayout | layout,
|  | kBool | enable
| ) |  |

Enables buddied sensor multiplexing with automated parameter calculation.

Note
  Supported with G1, G2

Version
  Introduced in firmware 4.0.10.27

Parameters

  layout | GoLayout object.
  enable | kTRUE to enable, or kFALSE to disable.

Returns
  Operation status.