Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSurfaceGenerationFixedLength_SetTriggerExternalInputIndex | ( | GoSurfaceGeneration | surface,
|  | k32s | index
| ) |  |

Sets the external input index to trigger surface capturing.

Note
  Supported with G2, G3

Version
  Introduced in firmware 5.2.1.110

Parameters

  surface | GoSurfaceGeneration object.
  index | External digital input index.

Returns
  Operation status.