Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSensor_UploadFile | ( | GoSensor | sensor,
|  | const kChar * | sourcePath,
|  | const kChar * | destName
| ) |  |

Uploads a file to the connected sensor.

The following is a list of macros representing common files used in this operation:

- GO_SENSOR_LIVE_JOB - Represents "_live.job".
- GO_SENSOR_LIVE_REPLAY - Represents the recording file, "_live.rec".

WARNING! This operation writes to flash storage. Review the user manual for implications.

Version
  Introduced in firmware 4.0.10.27

Parameters

  sensor | GoSensor object.
  sourcePath | Source file system path for the file to be uploaded.
  destName | Destination name for the uploaded file (maximum 63 characters).

Returns
  Operation status.

Remarks
  Calling this function will result in writing operations to flash storage if the destination is not a live file. Should the process be disrupted due to power loss or other factors, the sensor may enter Rescue mode.