Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSensor_SetAlignmentReference | ( | GoSensor | sensor,
|  | GoAlignmentRef | reference
| ) |  |

Sets the alignment reference of the sensor.

Version
  Introduced in firmware 4.0.10.27

Parameters

  sensor | GoSensor object.
  reference | The alignment reference value to set.

Returns
  Operation status.