Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoAcceleratorMgr_GetPortRange | ( | GoAcceleratorMgr | manager,
|  | k16u * | startPort,
|  | k16u * | endPort
| ) |  |

Get the range of port numbers to assign to accelerated sensors.

The ports within the port range are used by the Accelerator Manager to allocate ports for the accelerated sensors.

Version
  Introduced in firmware 5.2.18.3

Parameters

  manager | GoAcceleratorMgr object.
  startPort | Returns the starting port number in the range
  endPort | Returns the last port number in the range.

Returns
  Operation status.