Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoControl_BeginSnapshot | ( | GoControl | control | ) |

Sends a snapshot command to a sensor with the currently selected input source, but doesn't wait for the response.

Use the GoControl_EndSnapshot function to wait for the sensor's reply.

Version
  Introduced in firmware 5.2.1.x

Parameters

  control | GoControl object.

Returns
  Operation status.

See also
  GoControl_EndSnapshot, GoControl_SetInputSource, GoControl_GetInputSource