Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoControl_BeginAlignment | ( | GoControl | control | ) |

Sends a alignment command to a sensor, but doesn't wait for the response.

Use the GoControl_EndAlignment function to wait for the sensor's reply.

Version
  Introduced in firmware 4.0.10.27

Parameters

  control | GoControl object.

Returns
  Operation status.

See also
  GoControl_EndAlignment