Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoControl_SetInputSource | ( | GoControl | control,
|  | GoInputSource | source
| ) |  |

Sets the sensor's data input source.

Version
  Introduced in firmware 4.0.10.27

Parameters

  control | GoControl object.
  source | The input source to set.

Returns
  Operation status.