Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

k64f GoLayout_MultiplexSinglePeriod | ( | GoLayout | layout | ) |

Returns a value representing the multiplexing period in a single device sensor configuration.

(microseconds)

Note
  Supported with G1, G2

Version
  Introduced in firmware 4.0.10.27

Parameters

  layout | GoLayout object.

Returns
  Single device multiplexing period.