Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

k64f GoSetup_BackCameraExposureLimitMin | ( | GoSetup | setup,
|  | GoRole | role
| ) |  |

Gets the minimum valid value for the back camara exposure setting.

Version
  Introduced in firmware 4.6.0.140

Parameters

  setup | GoSetup object.
  role | Determines which device to retrieve the value from. Use GO_ROLE_MAIN or GOROLE_BUDDYIDX(buddyidx). See GoRole for more details.

Returns
  Minimum valid auxiliary exposure value (microseconds).