Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoAdvanced_SetSpotThreshold | ( | GoAdvanced | advanced,
|  | k32u | value
| ) |  |

Sets the spot threshold.

Note
  Supported with G1, G2

Version
  Introduced in firmware 4.6.1.140

Parameters

  advanced | GoAdvanced object.
  value | Spot threshold.

Returns
  Operation status.