Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSetup_EnableYDecimation | ( | GoSetup | setup,
|  | kBool | enable
| ) |  |

Sets the status of y-direction decimation.

Note
  Supported with G1, G2

Version
  Introduced in firmware 4.1.3.106

Parameters

  setup | GoSetup object.
  enable | Enable or disable y-decimation

Returns
  Operation status.