Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSurfaceBox_SetAsymmetryDetectionType | ( | GoSurfaceBox | tool,
|  | GoBoxAsymmetryType | value
| ) |  |

Sets the asymmetry detection type.

Note
  Supported with G2, G3

Version
  Introduced in firmware 4.4.4.14

Parameters

  tool | GoSurfaceBox object.
  value | The asymmetry detection type to set.

Returns
  Operation status.