Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages
GoSurfaceToolUtils.h
Go to the documentation of this file.
1 /// @cond (Gocator_2x00 || Gocator_3x00)
2 /**
3 * @file GoSurfaceToolUtils.h
4 * @brief Declares all surface tools and their related classes.
5 *
6 * @internal
7 * Copyright (C) 2016-2018 by LMI Technologies Inc.
8 * Licensed under the MIT License.
9 * Redistributed files must retain the above copyright notice.
10 */
11
12 #ifndef GO_SURFACE_TOOL_UTILS_H
13 #define GO_SURFACE_TOOL_UTILS_H
14
15 #include <GoSdk/GoSdkDef.h>
16 #include <GoSdk/GoUtils.h>
17 #include <GoSdk/Tools/GoFeature.h>
18
19 kBeginHeader()
20
21 /**
22 * @class GoSurfaceRegion2d
23 * @extends kObject
24 * @ingroup GoSdk-SurfaceTools
25 * @brief Represents a two dimensional surface tool region.
26 */
27 typedef kObject GoSurfaceRegion2d;
28
29 /**
30 * Sets the X position.
31 *
32 * @public @memberof GoSurfaceRegion2d
33 * @version Introduced in firmware 4.0.10.27
34 * @param region GoSurfaceRegion2d object.
35 * @param x The X position to set.(mm)
36 * @return Operation status.
37 */
38 GoFx(kStatus) GoSurfaceRegion2d_SetX(GoSurfaceRegion2d region, k64f x);
39
40 /**
41 * Gets the X position.
42 *
43 * @public @memberof GoSurfaceRegion2d
44 * @version Introduced in firmware 4.0.10.27
45 * @param region GoSurfaceRegion2d object.
46 * @return The X position of the region.(mm)
47 */
48 GoFx(k64f) GoSurfaceRegion2d_X(GoSurfaceRegion2d region);
49
50 /**
51 * Sets the Y position.
52 *
53 * @public @memberof GoSurfaceRegion2d
54 * @version Introduced in firmware 4.0.10.27
55 * @param region GoSurfaceRegion2d object.
56 * @param value The Y position to set.(mm)
57 * @return Operation status.
58 */
59 GoFx(kStatus) GoSurfaceRegion2d_SetY(GoSurfaceRegion2d region, k64f value);
60
61 /**
62 * Gets the Y position.
63 *
64 * @public @memberof GoSurfaceRegion2d
65 * @version Introduced in firmware 4.0.10.27
66 * @param region GoSurfaceRegion2d object.
67 * @return The Y position of the region.(mm)
68 */
69 GoFx(k64f) GoSurfaceRegion2d_Y(GoSurfaceRegion2d region);
70
71 /**
72 * Sets the width.
73 *
74 * @public @memberof GoSurfaceRegion2d
75 * @version Introduced in firmware 4.0.10.27
76 * @param region GoSurfaceRegion2d object.
77 * @param width The width to set.(mm)
78 * @return Operation status.
79 */
80 GoFx(kStatus) GoSurfaceRegion2d_SetWidth(GoSurfaceRegion2d region, k64f width);
81
82 /**
83 * Gets the width.
84 *
85 * @public @memberof GoSurfaceRegion2d
86 * @version Introduced in firmware 4.0.10.27
87 * @param region GoSurfaceRegion2d object.
88 * @return The width of the region.(mm)
89 */
90 GoFx(k64f) GoSurfaceRegion2d_Width(GoSurfaceRegion2d region);
91
92 /**
93 * Sets the length.
94 *
95 * @public @memberof GoSurfaceRegion2d
96 * @version Introduced in firmware 4.0.10.27
97 * @param region GoSurfaceRegion2d object.
98 * @param length The length to set.(mm)
99 * @return Operation status.
100 */
101 GoFx(kStatus) GoSurfaceRegion2d_SetLength(GoSurfaceRegion2d region, k64f length);
102
103 /**
104 * Gets the length.
105 *
106 * @public @memberof GoSurfaceRegion2d
107 * @version Introduced in firmware 4.0.10.27
108 * @param region GoSurfaceRegion2d object.
109 * @return The length of the region.(mm)
110 */
111 GoFx(k64f) GoSurfaceRegion2d_Length(GoSurfaceRegion2d region);
112
113 /**
114 * Sets the length.
115 *
116 * @public @memberof GoSurfaceRegion2d
117 * @version Introduced in firmware 4.0.10.27
118 * @param region GoSurfaceRegion2d object.
119 * @param zAngle The zAngle to set.(degrees)
120 * @return Operation status.
121 */
122 GoFx(kStatus) GoSurfaceRegion2d_SetZAngle(GoSurfaceRegion2d region, k64f zAngle);
123
124 /**
125 * Gets the length.
126 *
127 * @public @memberof GoSurfaceRegion2d
128 * @version Introduced in firmware 4.0.10.27
129 * @param region GoSurfaceRegion2d object.
130 * @return The zAngle of the region.(degrees)
131 */
132 GoFx(k64f) GoSurfaceRegion2d_ZAngle(GoSurfaceRegion2d region);
133
134
135 /**
136 * @class GoRegion3d
137 * @extends kObject
138 * @ingroup GoSdk-SurfaceTools
139 * @brief Represents a three dimensional surface region.
140 */
141 typedef kObject GoRegion3d;
142
143 /**
144 * Sets the X position.
145 *
146 * @public @memberof GoRegion3d
147 * @version Introduced in firmware 4.0.10.27
148 * @param region GoRegion3d object.
149 * @param x The X position to set.(mm)
150 * @return Operation status.
151 */
152 GoFx(kStatus) GoRegion3d_SetX(GoRegion3d region, k64f x);
153
154 /**
155 * Gets the X position.
156 *
157 * @public @memberof GoRegion3d
158 * @version Introduced in firmware 4.0.10.27
159 * @param region GoRegion3d object.
160 * @return The X position of the region.(mm)
161 */
162 GoFx(k64f) GoRegion3d_X(GoRegion3d region);
163
164 /**
165 * Sets the Y position.
166 *
167 * @public @memberof GoRegion3d
168 * @version Introduced in firmware 4.0.10.27
169 * @param region GoRegion3d object.
170 * @param value The Y position to set.(mm)
171 * @return Operation status.
172 */
173 GoFx(kStatus) GoRegion3d_SetY(GoRegion3d region, k64f value);
174
175 /**
176 * Gets the Y position.
177 *
178 * @public @memberof GoRegion3d
179 * @version Introduced in firmware 4.0.10.27
180 * @param region GoRegion3d object.
181 * @return The Y position of the region.(mm)
182 */
183 GoFx(k64f) GoRegion3d_Y(GoRegion3d region);
184
185 /**
186 * Sets the Z-position.
187 *
188 * @public @memberof GoRegion3d
189 * @version Introduced in firmware 4.0.10.27
190 * @param region GoRegion3d object.
191 * @param z The Z-position to set.(mm)
192 * @return Operation status.
193 */
194 GoFx(kStatus) GoRegion3d_SetZ(GoRegion3d region, k64f z);
195
196 /**
197 * Gets the Z-position.
198 *
199 * @public @memberof GoRegion3d
200 * @version Introduced in firmware 4.0.10.27
201 * @param region GoRegion3d object.
202 * @return The Z-position of the region.(mm)
203 */
204 GoFx(k64f) GoRegion3d_Z(GoRegion3d region);
205
206 /**
207 * Sets the width.
208 *
209 * @public @memberof GoRegion3d
210 * @version Introduced in firmware 4.0.10.27
211 * @param region GoRegion3d object.
212 * @param width The width to set.(mm)
213 * @return Operation status.
214 */
215 GoFx(kStatus) GoRegion3d_SetWidth(GoRegion3d region, k64f width);
216
217 /**
218 * Gets the width.
219 *
220 * @public @memberof GoRegion3d
221 * @version Introduced in firmware 4.0.10.27
222 * @param region GoRegion3d object.
223 * @return The width of the region.(mm)
224 */
225 GoFx(k64f) GoRegion3d_Width(GoRegion3d region);
226
227 /**
228 * Sets the length.
229 *
230 * @public @memberof GoRegion3d
231 * @version Introduced in firmware 4.0.10.27
232 * @param region GoRegion3d object.
233 * @param length The length to set.(mm)
234 * @return Operation status.
235 */
236 GoFx(kStatus) GoRegion3d_SetLength(GoRegion3d region, k64f length);
237
238 /**
239 * Gets the length.
240 *
241 * @public @memberof GoRegion3d
242 * @version Introduced in firmware 4.0.10.27
243 * @param region GoRegion3d object.
244 * @return The length of the region.(mm)
245 */
246 GoFx(k64f) GoRegion3d_Length(GoRegion3d region);
247
248 /**
249 * Sets the height.
250 *
251 * @public @memberof GoRegion3d
252 * @version Introduced in firmware 4.0.10.27
253 * @param region GoRegion3d object.
254 * @param height The height to set.(mm)
255 * @return Operation status.
256 */
257 GoFx(kStatus) GoRegion3d_SetHeight(GoRegion3d region, k64f height);
258
259 /**
260 * Gets the height.
261 *
262 * @public @memberof GoRegion3d
263 * @version Introduced in firmware 4.0.10.27
264 * @param region GoRegion3d object.
265 * @return The height of the region.(mm)
266 */
267 GoFx(k64f) GoRegion3d_Height(GoRegion3d region);
268
269 /**
270 * Sets the height.
271 *
272 * @public @memberof GoRegion3d
273 * @version Introduced in firmware 4.0.10.27
274 * @param region GoRegion3d object.
275 * @param zAngle The zAngle to set.(degrees)
276 * @return Operation status.
277 */
278 GoFx(kStatus) GoRegion3d_SetZAngle(GoRegion3d region, k64f zAngle);
279
280 /**
281 * Gets the height.
282 *
283 * @public @memberof GoRegion3d
284 * @version Introduced in firmware 4.0.10.27
285 * @param region GoRegion3d object.
286 * @return The zAngle of the region.(degrees)
287 */
288 GoFx(k64f) GoRegion3d_ZAngle(GoRegion3d region);
289
290
291 /**
292 * @class GoCylinderRegion
293 * @extends kObject
294 * @ingroup GoSdk-SurfaceTools
295 * @brief Represents a cylinder region for select surface tools.
296 */
297 typedef kObject GoCylinderRegion;
298
299 /**
300 * Sets the X position.
301 *
302 * @public @memberof GoCylinderRegion
303 * @version Introduced in firmware 4.0.10.27
304 * @param region GoCylinderRegion object.
305 * @param x The X position to set.(mm)
306 * @return Operation status.
307 */
308 GoFx(kStatus) GoCylinderRegion_SetX(GoCylinderRegion region, k64f x);
309
310 /**
311 * Gets the X position.
312 *
313 * @public @memberof GoCylinderRegion
314 * @version Introduced in firmware 4.0.10.27
315 * @param region GoCylinderRegion object.
316 * @return The X position of the region.(mm)
317 */
318 GoFx(k64f) GoCylinderRegion_X(GoCylinderRegion region);
319
320 /**
321 * Sets the Y position.
322 *
323 * @public @memberof GoCylinderRegion
324 * @version Introduced in firmware 4.0.10.27
325 * @param region GoCylinderRegion object.
326 * @param value The Y position to set.(mm)
327 * @return Operation status.
328 */
329 GoFx(kStatus) GoCylinderRegion_SetY(GoCylinderRegion region, k64f value);
330
331 /**
332 * Gets the Y position.
333 *
334 * @public @memberof GoCylinderRegion
335 * @version Introduced in firmware 4.0.10.27
336 * @param region GoCylinderRegion object.
337 * @return The Y position of the region.(mm)
338 */
339 GoFx(k64f) GoCylinderRegion_Y(GoCylinderRegion region);
340
341 /**
342 * Sets the Z-position.
343 *
344 * @public @memberof GoCylinderRegion
345 * @version Introduced in firmware 4.0.10.27
346 * @param region GoCylinderRegion object.
347 * @param z The Z-position to set.(mm)
348 * @return Operation status.
349 */
350 GoFx(kStatus) GoCylinderRegion_SetZ(GoCylinderRegion region, k64f z);
351
352 /**
353 * Gets the Z-position.
354 *
355 * @public @memberof GoCylinderRegion
356 * @version Introduced in firmware 4.0.10.27
357 * @param region GoCylinderRegion object.
358 * @return The Z-position of the region.(mm)
359 */
360 GoFx(k64f) GoCylinderRegion_Z(GoCylinderRegion region);
361
362 /**
363 * Sets the radius.
364 *
365 * @public @memberof GoCylinderRegion
366 * @version Introduced in firmware 4.0.10.27
367 * @param region GoCylinderRegion object.
368 * @param value The radius to set.(mm)
369 * @return Operation status.
370 */
371 GoFx(kStatus) GoCylinderRegion_SetRadius(GoCylinderRegion region, k64f value);
372
373 /**
374 * Gets the radius.
375 *
376 * @public @memberof GoCylinderRegion
377 * @version Introduced in firmware 4.0.10.27
378 * @param region GoCylinderRegion object.
379 * @return The radius of the region.(mm)
380 */
381 GoFx(k64f) GoCylinderRegion_Radius(GoCylinderRegion region);
382
383 /**
384 * Sets the height.
385 *
386 * @public @memberof GoCylinderRegion
387 * @version Introduced in firmware 4.0.10.27
388 * @param region GoCylinderRegion object.
389 * @param value The height to set.(mm)
390 * @return Operation status.
391 */
392 GoFx(kStatus) GoCylinderRegion_SetHeight(GoCylinderRegion region, k64f value);
393
394 /**
395 * Gets the height.
396 *
397 * @public @memberof GoCylinderRegion
398 * @version Introduced in firmware 4.0.10.27
399 * @param region GoCylinderRegion object.
400 * @return The height of the region.(mm)
401 */
402 GoFx(k64f) GoCylinderRegion_Height(GoCylinderRegion region);
403
404
405 /**
406 * @class GoSurfaceFeature
407 * @extends kObject
408 * @ingroup GoSdk-SurfaceTools
409 * @brief Represents a surface feature for select surface tools.
410 */
411 typedef kObject GoSurfaceFeature;
412
413 /**
414 * Gets the surface feature type.
415 *
416 * @public @memberof GoSurfaceFeature
417 * @version Introduced in firmware 4.0.10.27
418 * @param feature GoSurfaceFeature object.
419 * @return The surface feature type.
420 */
421 GoFx(GoSurfaceFeatureType) GoSurfaceFeature_Type(GoSurfaceFeature feature);
422
423 /**
424 * Sets the surface feature type.
425 *
426 * @public @memberof GoSurfaceFeature
427 * @version Introduced in firmware 4.0.10.27
428 * @param feature GoSurfaceFeature object.
429 * @param type The feature type value to set.
430 * @return Operation status.
431 */
432 GoFx(kStatus) GoSurfaceFeature_SetType(GoSurfaceFeature feature, GoSurfaceFeatureType type);
433
434 /**
435 * Gets the current state the surface feature region.
436 *
437 * @public @memberof GoSurfaceFeature
438 * @version Introduced in firmware 4.0.10.27
439 * @param feature GoSurfaceFeature object.
440 * @return kTRUE if enabled and kFALSE if disabled.
441 */
442 GoFx(kBool) GoSurfaceFeature_RegionEnabled(GoSurfaceFeature feature);
443
444 /**
445 * Enable or disable the surface feature region.
446 *
447 * @public @memberof GoSurfaceFeature
448 * @version Introduced in firmware 4.0.10.27
449 * @param feature GoSurfaceFeature object.
450 * @param enable kTRUE to enable, or kFALSE to disable.
451 * @return Operation status.
452 */
453 GoFx(kStatus) GoSurfaceFeature_EnableRegion(GoSurfaceFeature feature, kBool enable);
454
455 /**
456 * Gets the 3d region for the feature.
457 *
458 * @public @memberof GoSurfaceFeature
459 * @version Introduced in firmware 4.0.10.27
460 * @param feature GoSurfaceFeature object.
461 * @return A GoRegion3d object.
462 */
463 GoFx(GoRegion3d) GoSurfaceFeature_Region(GoSurfaceFeature feature);
464
465
466 kEndHeader()
467 #include <GoSdk/Tools/GoSurfaceToolUtils.x.h>
468
469 #endif
470
471 /// @endcond
GoSurfaceRegion2d::GoSurfaceRegion2d_SetWidth
kStatus GoSurfaceRegion2d_SetWidth(GoSurfaceRegion2d region, k64f width)
Sets the width.
GoSurfaceRegion2d::GoSurfaceRegion2d_Length
k64f GoSurfaceRegion2d_Length(GoSurfaceRegion2d region)
Gets the length.
GoCylinderRegion::GoCylinderRegion_Y
k64f GoCylinderRegion_Y(GoCylinderRegion region)
Gets the Y position.
GoSurfaceFeatureType
Represents a surface feature type.
GoRegion3d::GoRegion3d_X
k64f GoRegion3d_X(GoRegion3d region)
Gets the X position.
GoRegion3d::GoRegion3d_SetHeight
kStatus GoRegion3d_SetHeight(GoRegion3d region, k64f height)
Sets the height.
GoRegion3d::GoRegion3d_SetLength
kStatus GoRegion3d_SetLength(GoRegion3d region, k64f length)
Sets the length.
GoCylinderRegion::GoCylinderRegion_Radius
k64f GoCylinderRegion_Radius(GoCylinderRegion region)
Gets the radius.
GoRegion3d::GoRegion3d_SetZ
kStatus GoRegion3d_SetZ(GoRegion3d region, k64f z)
Sets the Z-position.
GoSurfaceFeature::GoSurfaceFeature_Region
GoRegion3d GoSurfaceFeature_Region(GoSurfaceFeature feature)
Gets the 3d region for the feature.
GoCylinderRegion::GoCylinderRegion_X
k64f GoCylinderRegion_X(GoCylinderRegion region)
Gets the X position.
GoCylinderRegion::GoCylinderRegion_SetX
kStatus GoCylinderRegion_SetX(GoCylinderRegion region, k64f x)
Sets the X position.
GoCylinderRegion::GoCylinderRegion_Z
k64f GoCylinderRegion_Z(GoCylinderRegion region)
Gets the Z-position.
GoCylinderRegion::GoCylinderRegion_SetY
kStatus GoCylinderRegion_SetY(GoCylinderRegion region, k64f value)
Sets the Y position.
GoSurfaceRegion2d::GoSurfaceRegion2d_ZAngle
k64f GoSurfaceRegion2d_ZAngle(GoSurfaceRegion2d region)
Gets the length.
GoSurfaceFeature::GoSurfaceFeature_RegionEnabled
kBool GoSurfaceFeature_RegionEnabled(GoSurfaceFeature feature)
Gets the current state the surface feature region.
GoCylinderRegion
Represents a cylinder region for select surface tools.
GoUtils.h
Contains various helper functions.
GoRegion3d::GoRegion3d_Y
k64f GoRegion3d_Y(GoRegion3d region)
Gets the Y position.
GoSurfaceRegion2d::GoSurfaceRegion2d_Y
k64f GoSurfaceRegion2d_Y(GoSurfaceRegion2d region)
Gets the Y position.
GoCylinderRegion::GoCylinderRegion_SetZ
kStatus GoCylinderRegion_SetZ(GoCylinderRegion region, k64f z)
Sets the Z-position.
GoSurfaceRegion2d::GoSurfaceRegion2d_X
k64f GoSurfaceRegion2d_X(GoSurfaceRegion2d region)
Gets the X position.
GoSurfaceFeature::GoSurfaceFeature_Type
GoSurfaceFeatureType GoSurfaceFeature_Type(GoSurfaceFeature feature)
Gets the surface feature type.
GoSdkDef.h
Essential SDK declarations.
GoSurfaceRegion2d::GoSurfaceRegion2d_SetX
kStatus GoSurfaceRegion2d_SetX(GoSurfaceRegion2d region, k64f x)
Sets the X position.
GoFeature.h
Declares the GoFeature class.
GoCylinderRegion::GoCylinderRegion_Height
k64f GoCylinderRegion_Height(GoCylinderRegion region)
Gets the height.
GoSurfaceRegion2d
Represents a two dimensional surface tool region.
GoSurfaceRegion2d::GoSurfaceRegion2d_SetLength
kStatus GoSurfaceRegion2d_SetLength(GoSurfaceRegion2d region, k64f length)
Sets the length.
GoRegion3d::GoRegion3d_SetWidth
kStatus GoRegion3d_SetWidth(GoRegion3d region, k64f width)
Sets the width.
GoSurfaceRegion2d::GoSurfaceRegion2d_SetY
kStatus GoSurfaceRegion2d_SetY(GoSurfaceRegion2d region, k64f value)
Sets the Y position.
GoRegion3d
Represents a three dimensional surface region.
GoRegion3d::GoRegion3d_Z
k64f GoRegion3d_Z(GoRegion3d region)
Gets the Z-position.
GoRegion3d::GoRegion3d_SetX
kStatus GoRegion3d_SetX(GoRegion3d region, k64f x)
Sets the X position.
GoRegion3d::GoRegion3d_ZAngle
k64f GoRegion3d_ZAngle(GoRegion3d region)
Gets the height.
GoSurfaceFeature::GoSurfaceFeature_SetType
kStatus GoSurfaceFeature_SetType(GoSurfaceFeature feature, GoSurfaceFeatureType type)
Sets the surface feature type.
GoRegion3d::GoRegion3d_Width
k64f GoRegion3d_Width(GoRegion3d region)
Gets the width.
GoCylinderRegion::GoCylinderRegion_SetHeight
kStatus GoCylinderRegion_SetHeight(GoCylinderRegion region, k64f value)
Sets the height.
kObject
kStatus
GoRegion3d::GoRegion3d_Height
k64f GoRegion3d_Height(GoRegion3d region)
Gets the height.
GoRegion3d::GoRegion3d_SetZAngle
kStatus GoRegion3d_SetZAngle(GoRegion3d region, k64f zAngle)
Sets the height.
GoSurfaceFeature::GoSurfaceFeature_EnableRegion
kStatus GoSurfaceFeature_EnableRegion(GoSurfaceFeature feature, kBool enable)
Enable or disable the surface feature region.
k64f
GoCylinderRegion::GoCylinderRegion_SetRadius
kStatus GoCylinderRegion_SetRadius(GoCylinderRegion region, k64f value)
Sets the radius.
kBool
GoSurfaceFeature
Represents a surface feature for select surface tools.
GoSurfaceRegion2d::GoSurfaceRegion2d_SetZAngle
kStatus GoSurfaceRegion2d_SetZAngle(GoSurfaceRegion2d region, k64f zAngle)
Sets the length.
GoRegion3d::GoRegion3d_Length
k64f GoRegion3d_Length(GoRegion3d region)
Gets the length.
GoSurfaceRegion2d::GoSurfaceRegion2d_Width
k64f GoSurfaceRegion2d_Width(GoSurfaceRegion2d region)
Gets the width.
GoRegion3d::GoRegion3d_SetY
kStatus GoRegion3d_SetY(GoRegion3d region, k64f value)
Sets the Y position.