Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoControl_AssignBuddies | ( | GoControl | control,
|  | const k32u * | buddyIds,
|  | kSize | count
| ) |  |

Start assigning multiple buddy sensors.

A zero count unassigns all buddies.

Version
  Introduced in firmware 4.6.2.95

Parameters

  control | GoControl object.
  buddyIds | Buddy device id array.
  count | 0 to Unassign all buddies; ELSE Number of buddies to assign.

Returns
  Operation status.