Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoDiscovery_GetExtendedInfo | ( | GoDiscovery | discovery,
|  | k32u | deviceId,
|  | GoDiscoveryExtInfo * | info,
|  | kAlloc | allocator
| ) |  |

Retrieves a sensor's information.

This function uses UDP broadcasts; the sensor and can be on a different subnet than the client.

Version
  Introduced in firmware 4.3.3.124

Parameters

  discovery | Discovery object.
  deviceId | Sensor device identifier (serial number).
  info | Receives sensor information.
  allocator | Memory allocator. In order to prevent memory leaks, the received information object should be destroyed when no longer used.

Returns
  Operation status.