Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kBool GoSetup_PreferMasterTimeEncoderEnabled | ( | GoSetup | setup | ) |

Gets whether the time and encoder values are preferred to come from the Master rather than from the sensor and its I/O port.

Version
  Introduced in firmware 4.8.2.76

Parameters

  setup | GoSetup object.

Returns
  kTRUE if enabled and kFALSE otherwise.