Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages
GoSurfaceToolUtils.h
Go to the documentation of this file.
1 /**
2 * @file GoSurfaceToolUtils.h
3 * @brief Declares all surface tools and their related classes.
4 *
5 * @internal
6 * Copyright (C) 2016-2022 by LMI Technologies Inc.
7 * Licensed under the MIT License.
8 * Redistributed files must retain the above copyright notice.
9 */
10
11 #ifndef GO_SURFACE_TOOL_UTILS_H
12 #define GO_SURFACE_TOOL_UTILS_H
13
14 #include <GoSdk/GoSdkDef.h>
15 #include <GoSdk/GoUtils.h>
16 #include <GoSdk/Tools/GoFeature.h>
17
18 /**
19 * @class GoSurfaceRegion2d
20 * @extends kObject
21 * @ingroup GoSdk-SurfaceTools
22 * @brief Represents a two dimensional surface tool region.
23 */
24 typedef kObject GoSurfaceRegion2d;
25
26 /**
27 * Sets the X position.
28 *
29 * @public @memberof GoSurfaceRegion2d
30 * @note Supported with G2, G3
31 * @version Introduced in firmware 4.0.10.27
32 * @param region GoSurfaceRegion2d object.
33 * @param x The X position to set.(mm)
34 * @return Operation status.
35 */
36 GoFx(kStatus) GoSurfaceRegion2d_SetX(GoSurfaceRegion2d region, k64f x);
37
38 /**
39 * Gets the X position.
40 *
41 * @public @memberof GoSurfaceRegion2d
42 * @note Supported with G2, G3
43 * @version Introduced in firmware 4.0.10.27
44 * @param region GoSurfaceRegion2d object.
45 * @return The X position of the region.(mm)
46 */
47 GoFx(k64f) GoSurfaceRegion2d_X(GoSurfaceRegion2d region);
48
49 /**
50 * Sets the Y position.
51 *
52 * @public @memberof GoSurfaceRegion2d
53 * @note Supported with G2, G3
54 * @version Introduced in firmware 4.0.10.27
55 * @param region GoSurfaceRegion2d object.
56 * @param value The Y position to set.(mm)
57 * @return Operation status.
58 */
59 GoFx(kStatus) GoSurfaceRegion2d_SetY(GoSurfaceRegion2d region, k64f value);
60
61 /**
62 * Gets the Y position.
63 *
64 * @public @memberof GoSurfaceRegion2d
65 * @note Supported with G2, G3
66 * @version Introduced in firmware 4.0.10.27
67 * @param region GoSurfaceRegion2d object.
68 * @return The Y position of the region.(mm)
69 */
70 GoFx(k64f) GoSurfaceRegion2d_Y(GoSurfaceRegion2d region);
71
72 /**
73 * Sets the width.
74 *
75 * @public @memberof GoSurfaceRegion2d
76 * @note Supported with G2, G3
77 * @version Introduced in firmware 4.0.10.27
78 * @param region GoSurfaceRegion2d object.
79 * @param width The width to set.(mm)
80 * @return Operation status.
81 */
82 GoFx(kStatus) GoSurfaceRegion2d_SetWidth(GoSurfaceRegion2d region, k64f width);
83
84 /**
85 * Gets the width.
86 *
87 * @public @memberof GoSurfaceRegion2d
88 * @note Supported with G2, G3
89 * @version Introduced in firmware 4.0.10.27
90 * @param region GoSurfaceRegion2d object.
91 * @return The width of the region.(mm)
92 */
93 GoFx(k64f) GoSurfaceRegion2d_Width(GoSurfaceRegion2d region);
94
95 /**
96 * Sets the length.
97 *
98 * @public @memberof GoSurfaceRegion2d
99 * @note Supported with G2, G3
100 * @version Introduced in firmware 4.0.10.27
101 * @param region GoSurfaceRegion2d object.
102 * @param length The length to set.(mm)
103 * @return Operation status.
104 */
105 GoFx(kStatus) GoSurfaceRegion2d_SetLength(GoSurfaceRegion2d region, k64f length);
106
107 /**
108 * Gets the length.
109 *
110 * @public @memberof GoSurfaceRegion2d
111 * @note Supported with G2, G3
112 * @version Introduced in firmware 4.0.10.27
113 * @param region GoSurfaceRegion2d object.
114 * @return The length of the region.(mm)
115 */
116 GoFx(k64f) GoSurfaceRegion2d_Length(GoSurfaceRegion2d region);
117
118 /**
119 * Sets the length.
120 *
121 * @public @memberof GoSurfaceRegion2d
122 * @note Supported with G2, G3
123 * @version Introduced in firmware 4.0.10.27
124 * @param region GoSurfaceRegion2d object.
125 * @param zAngle The zAngle to set.(degrees)
126 * @return Operation status.
127 */
128 GoFx(kStatus) GoSurfaceRegion2d_SetZAngle(GoSurfaceRegion2d region, k64f zAngle);
129
130 /**
131 * Gets the length.
132 *
133 * @public @memberof GoSurfaceRegion2d
134 * @note Supported with G2, G3
135 * @version Introduced in firmware 4.0.10.27
136 * @param region GoSurfaceRegion2d object.
137 * @return The zAngle of the region.(degrees)
138 */
139 GoFx(k64f) GoSurfaceRegion2d_ZAngle(GoSurfaceRegion2d region);
140
141
142 /**
143 * @class GoRegion3d
144 * @extends kObject
145 * @note Supported with G2, G3
146 * @ingroup GoSdk-SurfaceTools
147 * @brief Represents a three dimensional surface region.
148 */
149 typedef kObject GoRegion3d;
150
151 /**
152 * Sets the X position.
153 *
154 * @public @memberof GoRegion3d
155 * @note Supported with G2, G3
156 * @version Introduced in firmware 4.0.10.27
157 * @param region GoRegion3d object.
158 * @param x The X position to set.(mm)
159 * @return Operation status.
160 */
161 GoFx(kStatus) GoRegion3d_SetX(GoRegion3d region, k64f x);
162
163 /**
164 * Gets the X position.
165 *
166 * @public @memberof GoRegion3d
167 * @note Supported with G2, G3
168 * @version Introduced in firmware 4.0.10.27
169 * @param region GoRegion3d object.
170 * @return The X position of the region.(mm)
171 */
172 GoFx(k64f) GoRegion3d_X(GoRegion3d region);
173
174 /**
175 * Sets the Y position.
176 *
177 * @public @memberof GoRegion3d
178 * @note Supported with G2, G3
179 * @version Introduced in firmware 4.0.10.27
180 * @param region GoRegion3d object.
181 * @param value The Y position to set.(mm)
182 * @return Operation status.
183 */
184 GoFx(kStatus) GoRegion3d_SetY(GoRegion3d region, k64f value);
185
186 /**
187 * Gets the Y position.
188 *
189 * @public @memberof GoRegion3d
190 * @note Supported with G2, G3
191 * @version Introduced in firmware 4.0.10.27
192 * @param region GoRegion3d object.
193 * @return The Y position of the region.(mm)
194 */
195 GoFx(k64f) GoRegion3d_Y(GoRegion3d region);
196
197 /**
198 * Sets the Z-position.
199 *
200 * @public @memberof GoRegion3d
201 * @note Supported with G2, G3
202 * @version Introduced in firmware 4.0.10.27
203 * @param region GoRegion3d object.
204 * @param z The Z-position to set.(mm)
205 * @return Operation status.
206 */
207 GoFx(kStatus) GoRegion3d_SetZ(GoRegion3d region, k64f z);
208
209 /**
210 * Gets the Z-position.
211 *
212 * @public @memberof GoRegion3d
213 * @note Supported with G2, G3
214 * @version Introduced in firmware 4.0.10.27
215 * @param region GoRegion3d object.
216 * @return The Z-position of the region.(mm)
217 */
218 GoFx(k64f) GoRegion3d_Z(GoRegion3d region);
219
220 /**
221 * Sets the width.
222 *
223 * @public @memberof GoRegion3d
224 * @note Supported with G2, G3
225 * @version Introduced in firmware 4.0.10.27
226 * @param region GoRegion3d object.
227 * @param width The width to set.(mm)
228 * @return Operation status.
229 */
230 GoFx(kStatus) GoRegion3d_SetWidth(GoRegion3d region, k64f width);
231
232 /**
233 * Gets the width.
234 *
235 * @public @memberof GoRegion3d
236 * @note Supported with G2, G3
237 * @version Introduced in firmware 4.0.10.27
238 * @param region GoRegion3d object.
239 * @return The width of the region.(mm)
240 */
241 GoFx(k64f) GoRegion3d_Width(GoRegion3d region);
242
243 /**
244 * Sets the length.
245 *
246 * @public @memberof GoRegion3d
247 * @note Supported with G2, G3
248 * @version Introduced in firmware 4.0.10.27
249 * @param region GoRegion3d object.
250 * @param length The length to set.(mm)
251 * @return Operation status.
252 */
253 GoFx(kStatus) GoRegion3d_SetLength(GoRegion3d region, k64f length);
254
255 /**
256 * Gets the length.
257 *
258 * @public @memberof GoRegion3d
259 * @note Supported with G2, G3
260 * @version Introduced in firmware 4.0.10.27
261 * @param region GoRegion3d object.
262 * @return The length of the region.(mm)
263 */
264 GoFx(k64f) GoRegion3d_Length(GoRegion3d region);
265
266 /**
267 * Sets the height.
268 *
269 * @public @memberof GoRegion3d
270 * @note Supported with G2, G3
271 * @version Introduced in firmware 4.0.10.27
272 * @param region GoRegion3d object.
273 * @param height The height to set.(mm)
274 * @return Operation status.
275 */
276 GoFx(kStatus) GoRegion3d_SetHeight(GoRegion3d region, k64f height);
277
278 /**
279 * Gets the height.
280 *
281 * @public @memberof GoRegion3d
282 * @note Supported with G2, G3
283 * @version Introduced in firmware 4.0.10.27
284 * @param region GoRegion3d object.
285 * @return The height of the region.(mm)
286 */
287 GoFx(k64f) GoRegion3d_Height(GoRegion3d region);
288
289 /**
290 * Sets the height.
291 *
292 * @public @memberof GoRegion3d
293 * @note Supported with G2, G3
294 * @version Introduced in firmware 4.0.10.27
295 * @param region GoRegion3d object.
296 * @param zAngle The zAngle to set.(degrees)
297 * @return Operation status.
298 */
299 GoFx(kStatus) GoRegion3d_SetZAngle(GoRegion3d region, k64f zAngle);
300
301 /**
302 * Gets the height.
303 *
304 * @public @memberof GoRegion3d
305 * @note Supported with G2, G3
306 * @version Introduced in firmware 4.0.10.27
307 * @param region GoRegion3d object.
308 * @return The zAngle of the region.(degrees)
309 */
310 GoFx(k64f) GoRegion3d_ZAngle(GoRegion3d region);
311
312 /**
313 * @class GoPointSetRegion
314 * @extends kObject
315 * @note Supported with G2, G3
316 * @ingroup GoSdk-SurfaceTools
317 * @brief Represents a point set region.
318 */
319 typedef kObject GoPointSetRegion;
320
321 /**
322 * Sets constant-z value.
323 *
324 * @public @memberof GoPointSetRegion
325 * @note Supported with G2, G3
326 * @version Introduced in firmware 5.2.18.3
327 * @param region GoPointSetRegion object.
328 * @param constantZ Constant-z value
329 * @return Operation status
330 */
331 GoFx(kStatus) GoPointSetRegion_SetConstantZ(GoPointSetRegion region, k64f constantZ);
332
333 GoFx(const kPoint3d64f*) GoPointSetRegion_PointAt(GoPointSetRegion region, kSize index);
334
335 GoFx(kStatus) GoPointSetRegion_SetPointAt(GoPointSetRegion region, kSize index, const kPoint3d64f* point);
336
337 /**
338 * Disables constant-z.
339 *
340 * @public @memberof GoPointSetRegion
341 * @note Supported with G2, G3
342 * @version Introduced in firmware 5.2.18.3
343 * @param region GoPointSetRegion object.
344 * @return Operation status
345 */
346 GoFx(kStatus) GoPointSetRegion_DisableConstantZ(GoPointSetRegion region);
347
348 GoFx(kSize) GoPointSetRegion_PointCount(GoPointSetRegion region);
349
350 GoFx(kStatus) GoPointSetRegion_SetPointCount(GoPointSetRegion region, kSize count);
351
352 #if 0
353 /**
354 * Sets point values for the region.
355 *
356 * @public @memberof GoPointSetRegion
357 * @note Supported with G2, G3
358 * @version Introduced in firmware 5.2.18.3
359 * @param region GoPointSetRegion object.
360 * @param points kArrayList of kPoint3d64f. Values are copied.
361 * @return Operation status
362 */
363 GoFx(kStatus) GoPointSetRegion_SetPoints(GoPointSetRegion region, const kArrayList* points);
364
365 /**
366 * Gets point values for the region.
367 *
368 * @public @memberof GoPointSetRegion
369 * @note Supported with G2, G3
370 * @version Introduced in firmware 5.2.18.3
371 * @param region GoPointSetRegion object.
372 * @param points Pre-constructed kArrayList of kPoint3d64f. Values are copied.
373 * @return Operation status
374 */
375 GoFx(kStatus) GoPointSetRegion_Points(GoPointSetRegion region, kArrayList* points);
376 #endif
377
378 /**
379 * @class GoCylinderRegion
380 * @extends kObject
381 * @note Supported with G2, G3
382 * @ingroup GoSdk-SurfaceTools
383 * @brief Represents a cylinder region for select surface tools.
384 */
385 typedef kObject GoCylinderRegion;
386
387 /**
388 * Sets the X position.
389 *
390 * @public @memberof GoCylinderRegion
391 * @note Supported with G2, G3
392 * @version Introduced in firmware 4.0.10.27
393 * @param region GoCylinderRegion object.
394 * @param x The X position to set.(mm)
395 * @return Operation status.
396 */
397 GoFx(kStatus) GoCylinderRegion_SetX(GoCylinderRegion region, k64f x);
398
399 /**
400 * Gets the X position.
401 *
402 * @public @memberof GoCylinderRegion
403 * @note Supported with G2, G3
404 * @version Introduced in firmware 4.0.10.27
405 * @param region GoCylinderRegion object.
406 * @return The X position of the region.(mm)
407 */
408 GoFx(k64f) GoCylinderRegion_X(GoCylinderRegion region);
409
410 /**
411 * Sets the Y position.
412 *
413 * @public @memberof GoCylinderRegion
414 * @note Supported with G2, G3
415 * @version Introduced in firmware 4.0.10.27
416 * @param region GoCylinderRegion object.
417 * @param value The Y position to set.(mm)
418 * @return Operation status.
419 */
420 GoFx(kStatus) GoCylinderRegion_SetY(GoCylinderRegion region, k64f value);
421
422 /**
423 * Gets the Y position.
424 *
425 * @public @memberof GoCylinderRegion
426 * @note Supported with G2, G3
427 * @version Introduced in firmware 4.0.10.27
428 * @param region GoCylinderRegion object.
429 * @return The Y position of the region.(mm)
430 */
431 GoFx(k64f) GoCylinderRegion_Y(GoCylinderRegion region);
432
433 /**
434 * Sets the Z-position.
435 *
436 * @public @memberof GoCylinderRegion
437 * @note Supported with G2, G3
438 * @version Introduced in firmware 4.0.10.27
439 * @param region GoCylinderRegion object.
440 * @param z The Z-position to set.(mm)
441 * @return Operation status.
442 */
443 GoFx(kStatus) GoCylinderRegion_SetZ(GoCylinderRegion region, k64f z);
444
445 /**
446 * Gets the Z-position.
447 *
448 * @public @memberof GoCylinderRegion
449 * @note Supported with G2, G3
450 * @version Introduced in firmware 4.0.10.27
451 * @param region GoCylinderRegion object.
452 * @return The Z-position of the region.(mm)
453 */
454 GoFx(k64f) GoCylinderRegion_Z(GoCylinderRegion region);
455
456 /**
457 * Sets the radius.
458 *
459 * @public @memberof GoCylinderRegion
460 * @note Supported with G2, G3
461 * @version Introduced in firmware 4.0.10.27
462 * @param region GoCylinderRegion object.
463 * @param value The radius to set.(mm)
464 * @return Operation status.
465 */
466 GoFx(kStatus) GoCylinderRegion_SetRadius(GoCylinderRegion region, k64f value);
467
468 /**
469 * Gets the radius.
470 *
471 * @public @memberof GoCylinderRegion
472 * @note Supported with G2, G3
473 * @version Introduced in firmware 4.0.10.27
474 * @param region GoCylinderRegion object.
475 * @return The radius of the region.(mm)
476 */
477 GoFx(k64f) GoCylinderRegion_Radius(GoCylinderRegion region);
478
479 /**
480 * Sets the height.
481 *
482 * @public @memberof GoCylinderRegion
483 * @note Supported with G2, G3
484 * @version Introduced in firmware 4.0.10.27
485 * @param region GoCylinderRegion object.
486 * @param value The height to set.(mm)
487 * @return Operation status.
488 */
489 GoFx(kStatus) GoCylinderRegion_SetHeight(GoCylinderRegion region, k64f value);
490
491 /**
492 * Gets the height.
493 *
494 * @public @memberof GoCylinderRegion
495 * @note Supported with G2, G3
496 * @version Introduced in firmware 4.0.10.27
497 * @param region GoCylinderRegion object.
498 * @return The height of the region.(mm)
499 */
500 GoFx(k64f) GoCylinderRegion_Height(GoCylinderRegion region);
501
502
503 /**
504 * @class GoSurfaceFeature
505 * @extends kObject
506 * @ingroup GoSdk-SurfaceTools
507 * @brief Represents a surface feature for select surface tools.
508 */
509 typedef kObject GoSurfaceFeature;
510
511 /**
512 * Gets the surface feature type.
513 *
514 * @public @memberof GoSurfaceFeature
515 * @note Supported with G2, G3
516 * @version Introduced in firmware 4.0.10.27
517 * @param feature GoSurfaceFeature object.
518 * @return The surface feature type.
519 */
520 GoFx(GoSurfaceFeatureType) GoSurfaceFeature_Type(GoSurfaceFeature feature);
521
522 /**
523 * Sets the surface feature type.
524 *
525 * @public @memberof GoSurfaceFeature
526 * @note Supported with G2, G3
527 * @version Introduced in firmware 4.0.10.27
528 * @param feature GoSurfaceFeature object.
529 * @param type The feature type value to set.
530 * @return Operation status.
531 */
532 GoFx(kStatus) GoSurfaceFeature_SetType(GoSurfaceFeature feature, GoSurfaceFeatureType type);
533
534 /**
535 * Gets the current state the surface feature region.
536 *
537 * @public @memberof GoSurfaceFeature
538 * @note Supported with G2, G3
539 * @version Introduced in firmware 4.0.10.27
540 * @param feature GoSurfaceFeature object.
541 * @return kTRUE if enabled and kFALSE if disabled.
542 */
543 GoFx(kBool) GoSurfaceFeature_RegionEnabled(GoSurfaceFeature feature);
544
545 /**
546 * Enable or disable the surface feature region.
547 *
548 * @public @memberof GoSurfaceFeature
549 * @note Supported with G2, G3
550 * @version Introduced in firmware 4.0.10.27
551 * @param feature GoSurfaceFeature object.
552 * @param enable kTRUE to enable, or kFALSE to disable.
553 * @return Operation status.
554 */
555 GoFx(kStatus) GoSurfaceFeature_EnableRegion(GoSurfaceFeature feature, kBool enable);
556
557 /**
558 * Gets the 3d region for the feature.
559 *
560 * @public @memberof GoSurfaceFeature
561 * @note Supported with G2, G3
562 * @version Introduced in firmware 4.0.10.27
563 * @param feature GoSurfaceFeature object.
564 * @return A GoRegion3d object.
565 */
566 GoFx(GoRegion3d) GoSurfaceFeature_Region(GoSurfaceFeature feature);
567
568 #include <GoSdk/Tools/GoSurfaceToolUtils.x.h>
569
570 #endif
GoSurfaceRegion2d::GoSurfaceRegion2d_SetWidth
kStatus GoSurfaceRegion2d_SetWidth(GoSurfaceRegion2d region, k64f width)
Sets the width.
GoSurfaceRegion2d::GoSurfaceRegion2d_Length
k64f GoSurfaceRegion2d_Length(GoSurfaceRegion2d region)
Gets the length.
GoCylinderRegion::GoCylinderRegion_Y
k64f GoCylinderRegion_Y(GoCylinderRegion region)
Gets the Y position.
GoSurfaceFeatureType
Represents a surface feature type.
GoRegion3d::GoRegion3d_X
k64f GoRegion3d_X(GoRegion3d region)
Gets the X position.
GoRegion3d::GoRegion3d_SetHeight
kStatus GoRegion3d_SetHeight(GoRegion3d region, k64f height)
Sets the height.
GoRegion3d::GoRegion3d_SetLength
kStatus GoRegion3d_SetLength(GoRegion3d region, k64f length)
Sets the length.
GoCylinderRegion::GoCylinderRegion_Radius
k64f GoCylinderRegion_Radius(GoCylinderRegion region)
Gets the radius.
GoRegion3d::GoRegion3d_SetZ
kStatus GoRegion3d_SetZ(GoRegion3d region, k64f z)
Sets the Z-position.
GoSurfaceFeature::GoSurfaceFeature_Region
GoRegion3d GoSurfaceFeature_Region(GoSurfaceFeature feature)
Gets the 3d region for the feature.
GoCylinderRegion::GoCylinderRegion_X
k64f GoCylinderRegion_X(GoCylinderRegion region)
Gets the X position.
GoCylinderRegion::GoCylinderRegion_SetX
kStatus GoCylinderRegion_SetX(GoCylinderRegion region, k64f x)
Sets the X position.
kSize
GoCylinderRegion::GoCylinderRegion_Z
k64f GoCylinderRegion_Z(GoCylinderRegion region)
Gets the Z-position.
GoCylinderRegion::GoCylinderRegion_SetY
kStatus GoCylinderRegion_SetY(GoCylinderRegion region, k64f value)
Sets the Y position.
GoSurfaceRegion2d::GoSurfaceRegion2d_ZAngle
k64f GoSurfaceRegion2d_ZAngle(GoSurfaceRegion2d region)
Gets the length.
GoSurfaceFeature::GoSurfaceFeature_RegionEnabled
kBool GoSurfaceFeature_RegionEnabled(GoSurfaceFeature feature)
Gets the current state the surface feature region.
GoCylinderRegion
Represents a cylinder region for select surface tools.
GoUtils.h
Contains various helper functions.
GoRegion3d::GoRegion3d_Y
k64f GoRegion3d_Y(GoRegion3d region)
Gets the Y position.
GoSurfaceRegion2d::GoSurfaceRegion2d_Y
k64f GoSurfaceRegion2d_Y(GoSurfaceRegion2d region)
Gets the Y position.
GoCylinderRegion::GoCylinderRegion_SetZ
kStatus GoCylinderRegion_SetZ(GoCylinderRegion region, k64f z)
Sets the Z-position.
GoSurfaceRegion2d::GoSurfaceRegion2d_X
k64f GoSurfaceRegion2d_X(GoSurfaceRegion2d region)
Gets the X position.
GoPointSetRegion::GoPointSetRegion_SetConstantZ
kStatus GoPointSetRegion_SetConstantZ(GoPointSetRegion region, k64f constantZ)
Sets constant-z value.
GoSurfaceFeature::GoSurfaceFeature_Type
GoSurfaceFeatureType GoSurfaceFeature_Type(GoSurfaceFeature feature)
Gets the surface feature type.
GoSdkDef.h
Essential SDK declarations.
GoSurfaceRegion2d::GoSurfaceRegion2d_SetX
kStatus GoSurfaceRegion2d_SetX(GoSurfaceRegion2d region, k64f x)
Sets the X position.
GoFeature.h
Declares the GoFeature class.
GoCylinderRegion::GoCylinderRegion_Height
k64f GoCylinderRegion_Height(GoCylinderRegion region)
Gets the height.
GoSurfaceRegion2d
Represents a two dimensional surface tool region.
GoSurfaceRegion2d::GoSurfaceRegion2d_SetLength
kStatus GoSurfaceRegion2d_SetLength(GoSurfaceRegion2d region, k64f length)
Sets the length.
GoRegion3d::GoRegion3d_SetWidth
kStatus GoRegion3d_SetWidth(GoRegion3d region, k64f width)
Sets the width.
GoSurfaceRegion2d::GoSurfaceRegion2d_SetY
kStatus GoSurfaceRegion2d_SetY(GoSurfaceRegion2d region, k64f value)
Sets the Y position.
GoRegion3d
Represents a three dimensional surface region.
GoPointSetRegion
Represents a point set region.
GoPointSetRegion::GoPointSetRegion_DisableConstantZ
kStatus GoPointSetRegion_DisableConstantZ(GoPointSetRegion region)
Disables constant-z.
GoRegion3d::GoRegion3d_Z
k64f GoRegion3d_Z(GoRegion3d region)
Gets the Z-position.
GoRegion3d::GoRegion3d_SetX
kStatus GoRegion3d_SetX(GoRegion3d region, k64f x)
Sets the X position.
GoRegion3d::GoRegion3d_ZAngle
k64f GoRegion3d_ZAngle(GoRegion3d region)
Gets the height.
GoSurfaceFeature::GoSurfaceFeature_SetType
kStatus GoSurfaceFeature_SetType(GoSurfaceFeature feature, GoSurfaceFeatureType type)
Sets the surface feature type.
kArrayList
GoRegion3d::GoRegion3d_Width
k64f GoRegion3d_Width(GoRegion3d region)
Gets the width.
GoCylinderRegion::GoCylinderRegion_SetHeight
kStatus GoCylinderRegion_SetHeight(GoCylinderRegion region, k64f value)
Sets the height.
kObject
kStatus
GoRegion3d::GoRegion3d_Height
k64f GoRegion3d_Height(GoRegion3d region)
Gets the height.
GoRegion3d::GoRegion3d_SetZAngle
kStatus GoRegion3d_SetZAngle(GoRegion3d region, k64f zAngle)
Sets the height.
GoSurfaceFeature::GoSurfaceFeature_EnableRegion
kStatus GoSurfaceFeature_EnableRegion(GoSurfaceFeature feature, kBool enable)
Enable or disable the surface feature region.
k64f
GoCylinderRegion::GoCylinderRegion_SetRadius
kStatus GoCylinderRegion_SetRadius(GoCylinderRegion region, k64f value)
Sets the radius.
kBool
GoSurfaceFeature
Represents a surface feature for select surface tools.
kPoint3d64f
GoSurfaceRegion2d::GoSurfaceRegion2d_SetZAngle
kStatus GoSurfaceRegion2d_SetZAngle(GoSurfaceRegion2d region, k64f zAngle)
Sets the length.
GoRegion3d::GoRegion3d_Length
k64f GoRegion3d_Length(GoRegion3d region)
Gets the length.
GoSurfaceRegion2d::GoSurfaceRegion2d_Width
k64f GoSurfaceRegion2d_Width(GoSurfaceRegion2d region)
Gets the width.
GoRegion3d::GoRegion3d_SetY
kStatus GoRegion3d_SetY(GoRegion3d region, k64f value)
Sets the Y position.